# Didaktik 80 Emulation

Fuse supports Didaktik 80 (and Didaktik 40) emulation. It emulates the original version of the Didaktik 80, running MDOS 1 and with a WD2797 floppy controller.

The ROM file is not supplied with Fuse for macOS and so must be installed before the interface can be used. The expected file is a 14KB dump of the Didaktik 40/80 MDOS 1 ROM named didaktik80.rom and placed in the Fuse packages Contents/Resources directory.

See the Disk File Formats section for more details on supported disk file formats.

The Didaktik 80 may only be used with 16K, 48K and TC2048 emulation.

To press the Didaktik 80’s ‘SNAP’ button, choose the Machine > Didaktik SNAP menu option.